**CONTROL LED BY COMMUNICATION BETWEEN TWO ARDUINOS**

Serial communication between two Arduino, we can perform this on any two Arduino boards or another serial communicating device. Reciever receives serial data and Transmitter sends the serial data to other board or device.

COMPONENT :-

1. ARDUINO UNO
2. BUTTON
3. LED
4. RESISTOR

PROTEUS SIMULATION:-

